RD PORT VELA

* RS485 (RS-422 protocol, full duplex RS485 protocol)
* Baud rate: 57600 bps
* Data bits: 8
* No parity
* Stop bits: 1

**EN**

STP CABLE FOR RD PORTS

The RD ports transmit and receive audio and RS485 control signals. Below, the PIN-OUT is shown for an RJ45 connector and STP cable.

Note: do not connect an RD port to an RJ45 Ethernet port on a router or switch, the router or switch could be damaged.

**ES**

CABLE STP PARA PUERTOS RD

Los puertos RD transmiten y reciben señales de audio y de control RS485. A continuación, se muestra el PIN-OUT para un conector RJ45 y cable STP.

Nota: no conecte un puerto RD a un puerto de red RJ45 de un router o switch, el router o switch podría quedar dañado.

